## Façades made from thermally broken steel profiles – JANSEN VISS SG Façade

**Profile system**

Thermally broken mullion/transom construction consisting of rolled or drawn hollow steel profiles arranged on the room side with face widths of 50 or 60 mm and basic depths of 50 to 280 mm, in accordance with the structural requirements. The profile cross sections are to be checked by the contractor from a structural point of view. Proof of structural integrity must be provided before construction. The glazing is held by L-shaped or T-shaped glazing clips. The joint is sealed with a suitable sealing compound. The system has European Technical Approval - ETA 13/0015.

**Load-bearing structure**

Depending on the unit size, module size and type of construction, the load-bearing structure can be built either as a unitised construction (welded) and/or as a push-on construction (connecting spigot).

For the unitised construction, the transoms must be welded on all sides. For exposed constructions, the groove area in the mullion joint must be sealed by means of sealing compound. For the push-on construction, push-in or clip-in connecting spigots are available.

Local fixing anchors made from stainless steel with oval head screws with stainless steel flange are to be used as a connection between the load-bearing structure on the room side and the external pressure plates. Direct connections and thermal bridging must not arise between the internal load-bearing structure and the outer cover profiles.

**Drainage level**

Glazing weatherstrip made from continuous EPDM weatherstrips on the inside and outside. Weatherstrip joints overlap. The EPDM internal weatherstrips, which are to be installed on the isolators of the load-bearing structure by means of local perforation, block water and air movement for the glazing rebate. The horizontal weatherstrip with weatherstrip lips is continuous, whereby the top glass edge seal is covered. The vertical weatherstrip is inserted in between. The weatherstrip joints in the intersection points, T-joints and corner points must be sealed carefully using a suitable adhesive and sealing compound.

**Glass support and glass**

Load-bearing anchors made from stainless steel with aluminium rebate supports, a glass fibre-reinforced glass support profile or welded flat steel as well as plastic support blocks must be used in the glass support area for load transfer. The arrangement must be carried out in accordance with the regulations of the system and glazing manufacturer. Infill unit thicknesses from 30 to 70 mm can be used. In accordance with ETA 13/0015, only glass from Eckelt Glas GmbH may be used.

**Ventilation and drainage**

Rebate base ventilation and drainage of the glazing rebate is carried out to the outside, field by field, by means of deflector blocks in the transom area above the mullion area. The base point in the attachment to building structure area must be designed such that correct ventilation and drainage of the glazing rebate is guaranteed.

**Structural requirements**

The following minimum requirements for the façade must be strictly observed.

ETA based on ETAG 002

Air permeability in accordance with EN 12152   up to class AE

Watertightness in accordance with EN 12154 up to class RE 1200

Resistance to wind load, EN13116 up to 2 kN/m2

Impact resistance, EN14019 up to class E5/I5

Thermal transmittance in accordance with EN ISO 10077-2 from Uf > 0.84 W/m2K

